GPU inspection checklist
Date __________________________________   Time __________________________________
Station or ramp __________________________________   Operator name __________________________________
Unit number __________________________________   Hours __________________________________
Cables and connectors
	Item
	Pass
	Fail
	N/A

	Cable jacket has no cuts, crushing, burns or exposed wire
	☐
	☐
	☐

	Connector pins, plug and housing are clean and undamaged
	☐
	☐
	☐

	Strain relief at both ends is intact
	☐
	☐
	☐

	Cable storage or reel works and holds the cable off the ground
	☐
	☐
	☐

	Grounding connection and cable are in good condition
	☐
	☐
	☐



Unit
	Item
	Pass
	Fail
	N/A

	Housing, doors and guards are in place and secure
	☐
	☐
	☐

	Controls, switches and indicators work
	☐
	☐
	☐

	Emergency stop works
	☐
	☐
	☐

	Engine: oil, coolant and fuel levels, no leaks, or battery is secure and charged
	☐
	☐
	☐

	No fluid leaks under the unit
	☐
	☐
	☐

	Exhaust and cooling areas are clear
	☐
	☐
	☐



Mobility and safety
	Item
	Pass
	Fail
	N/A

	Tires and wheels are in good condition
	☐
	☐
	☐

	Brakes or chocks hold the unit
	☐
	☐
	☐

	Tow bar or hitch is secure
	☐
	☐
	☐

	Fire extinguisher is present and charged
	☐
	☐
	☐

	Warning labels and data plate are on and readable
	☐
	☐
	☐



Defects found and action taken
____________________________________________________________________________________________________
____________________________________________________________________________________________________
____________________________________________________________________________________________________
Taken out of service?  ☐ Yes   ☐ No        Reported to ______________________
Inspector signature __________________________________   Date __________________________________
Supervisor review __________________________________   Date __________________________________
A starting point. Adapt it to your equipment, your procedures and the rules that apply to you. Free template from portalbaseai.com
