Ladder inspection checklist
Date __________________________________   Location __________________________________
Inspector name __________________________________   Ladder ID or tag __________________________________
Ladder type __________________________________   Material __________________________________
Structure
	Item
	Pass
	Fail
	N/A

	Side rails are straight, with no cracks, bends or dents
	☐
	☐
	☐

	Rungs or steps are tight, secure and free of cracks
	☐
	☐
	☐

	Rungs and steps are clean and slip-resistant
	☐
	☐
	☐

	Spreaders and locks work, on a step ladder
	☐
	☐
	☐

	Rung locks, rope and pulley work, on an extension ladder
	☐
	☐
	☐



Feet and hardware
	Item
	Pass
	Fail
	N/A

	Feet or shoes are intact and grip
	☐
	☐
	☐

	Bolts, rivets and hardware are tight
	☐
	☐
	☐

	Labels and duty rating are readable
	☐
	☐
	☐



Condition
	Item
	Pass
	Fail
	N/A

	No oil, grease or mud on the rungs
	☐
	☐
	☐

	No paint or coating hiding a crack or damage
	☐
	☐
	☐

	No sign of an unsafe repair or modification
	☐
	☐
	☐

	Metal ladders are not used near electrical hazards
	☐
	☐
	☐



Defects found and action taken
____________________________________________________________________________________________________
____________________________________________________________________________________________________
____________________________________________________________________________________________________
Taken out of service?  ☐ Yes   ☐ No        Reported to ______________________
Inspector signature __________________________________   Date __________________________________
Supervisor review __________________________________   Date __________________________________
A starting point. Adapt it to your equipment, your procedures and the rules that apply to you. Free template from portalbaseai.com
