Machine guarding checklist
Date __________________________________   Time __________________________________
Area or line __________________________________   Machine name and ID __________________________________
Inspector __________________________________   Shift __________________________________
Guards
	Item
	Pass
	Fail
	N/A

	Every guard is in place and fastened
	☐
	☐
	☐

	Guards aren't bent, cracked or loose
	☐
	☐
	☐

	Pinch points, nip points and rotating parts are covered
	☐
	☐
	☐

	Guard openings don't let a hand reach the hazard
	☐
	☐
	☐

	No guard has been removed, taped open or bypassed
	☐
	☐
	☐



Interlocks and stops
	Item
	Pass
	Fail
	N/A

	Interlocks work and stop the machine when a guard opens
	☐
	☐
	☐

	Emergency stops are easy to reach and work
	☐
	☐
	☐

	Light curtains and sensors work, if fitted
	☐
	☐
	☐

	Machine can't restart on its own after a stop
	☐
	☐
	☐

	Controls are labeled and covered against accidental start
	☐
	☐
	☐



Labels and lockout
	Item
	Pass
	Fail
	N/A

	Warning labels are on and readable
	☐
	☐
	☐

	Lockout points are marked and reachable
	☐
	☐
	☐

	Energy sources are labeled
	☐
	☐
	☐

	Operating and lockout instructions are posted or at hand
	☐
	☐
	☐

	Floor around the machine is clear and the work area is lit
	☐
	☐
	☐



Defects found and action taken
____________________________________________________________________________________________________
____________________________________________________________________________________________________
____________________________________________________________________________________________________
Taken out of service?  ☐ Yes   ☐ No        Reported to ______________________
Inspector signature __________________________________   Date __________________________________
Supervisor review __________________________________   Date __________________________________
A starting point. Adapt it to your equipment, your procedures and the rules that apply to you. Free template from portalbaseai.com
