Belt loader inspection checklist
Date __________________________________   Time __________________________________
Station or ramp __________________________________   Operator name __________________________________
Unit number __________________________________   Hours __________________________________
Walkaround
	Item
	Pass
	Fail
	N/A

	Tires and wheels are in good condition
	☐
	☐
	☐

	Hydraulic hoses, fittings and cylinders have no leaks
	☐
	☐
	☐

	No fluid under the unit
	☐
	☐
	☐

	Guards and covers are in place and secure
	☐
	☐
	☐

	Positioning bumpers are intact and not hardened or torn
	☐
	☐
	☐

	Safety labels are on and readable
	☐
	☐
	☐



Conveyor
	Item
	Pass
	Fail
	N/A

	Belt is not frayed, torn or tracking to one side
	☐
	☐
	☐

	Rollers turn freely, with no jammed or missing parts
	☐
	☐
	☐

	Belt moves in both directions and stops when released
	☐
	☐
	☐

	Nothing is caught in the belt or the rollers
	☐
	☐
	☐



Controls and brakes
	Item
	Pass
	Fail
	N/A

	Emergency stop works
	☐
	☐
	☐

	Boom raises and lowers smoothly
	☐
	☐
	☐

	Service brake and parking brake work
	☐
	☐
	☐

	Steering works smoothly
	☐
	☐
	☐

	Horn, back-up alarm and lights work
	☐
	☐
	☐

	Beacon is on and visible
	☐
	☐
	☐

	Seat belt or restraint works, if fitted
	☐
	☐
	☐



Defects found and action taken
____________________________________________________________________________________________________
____________________________________________________________________________________________________
____________________________________________________________________________________________________
Taken out of service?  ☐ Yes   ☐ No        Reported to ______________________
Inspector signature __________________________________   Date __________________________________
Supervisor review __________________________________   Date __________________________________
A starting point. Adapt it to your equipment, your procedures and the rules that apply to you. Free template from portalbaseai.com
